W 00 1F 00
W 00 00 C4 -- activate spi 3w; 
W 00 01 05 -- enable NCO & SSBM (^2 interpolation)
W 00 02 00 -- pll 2x ; dac-phase set to 0 degrees
W 00 0F 03 -- NS enabled, minus 3dB enable
W 00 17 80
W 00 1F 04
W 00 07 E3 -- choose ILA initialization at 4th /A/
W 00 1F 02
W 00 00 30 -- full re-init; sync starts at '1'
